# **ZincBlue2 V1.2.13 Firmware and Software Update Instructions**

**Preparation for Update**

* Ensure ZincBlue2 UPS is powered on.
* Ensure all batteries are connected to ZincBlue2 UPS during firmware update.
* Ensure connectivity either directly to the ethernet port of the ZincBlue2 UPS, or through your network.

**Update Firmware**

* Log into the ZincBlue2 Software web application.
* Click the Settings tab.
* Click the Firmware page.
* To update the Firmware, click the Update Firmware button and drop the .pkg file into the dialog, or browse to the location on your computer.
* Click Start Update.
* When the Update Successful prompt is displayed, click Ok.
* Refresh browser.
* Login and verify version number by going to the Firmware page.

**Update Software**

* Log into the ZincBlue2 Software web application.
* Click the Settings tab.
* Click the Firmware page.
* To update the Software, click the Update Web UI button and drop the .tar file into the dialog, or browse to the location on your computer.
* Click Start Update.
* When the Update Successful prompt is displayed, click Ok.
* Refresh browser.
* Login and verify version number by going to the About page.